The Alfresco Contemporary System

A SLEEK YET MODERN STRUCTURE WITH A SUBTLE ELEGANCE

*Ideal for Big Span Verandas, Glass Rooms and Outdoor Dining Canopies*

The Contemporary Alfresco is a sleek yet modern structure that features a subtle elegance that will never go out of style due to its clean lines and minimal looking aluminium extrusions.

It can span up to 6 metres from the building and be manufactured in any length making it the ideal shade and shelter structure for any garden that boasts a striking, modern appearance.

The roof can be covered with 8mm toughened glass that offers a clear view of the sky.

The frame is made completely from strong aluminium extrusions which are naturally rust-resistant and are finished in Anthracite Grey Textured (RAL 7016) as standard. Hidden within the frame are integrated guttering and downpipes keeping the appearance of this structure smart and sharp.

* 6m Maximum Projection
* 6m Max Between Posts
* 800mm Max Between Bars
* 60 years Life Expectancy
* 10 years Guarantee
* 45 degrees Max Pitch
* 5 degrees Min Pitch
* 1 standard Colour

### Why Sell The Alfresco Contemporary System To Your Customers?

* **Striking Modern Appearance:** Making the contemporary Alfresco perfect for new builds and modern outdoor settings.
* **10 Year Guarantee:** The Contemporary Alfresco is supplied with a full 10 year guarantee and a 60 year life expectancy for the canopy frame which you can pass onto your customers.
* **Fully Aluminium Frame:** The canopy frame is made completely from aluminium which is naturally very strong and rust resistant making it perfect for outdoor use.
* **Toughened Glass:** The 8mm glass roof panels are toughened during manufacturing and achieve Class 1 BS EN 12600 for impact performance.
* **Low Maintenance:** The glass roof is low maintenance and the frame is made from aluminium which requires less maintenance than inferior materials such as PVC.
* **High Light Transmittance:**  All roof options offer a high light transmittance, keeping the area underneath well-lit.
* **6m Projection:** The Contemporary Alfresco can span up to an impressive 6 metres from the wall, enabling the Contemporary Alfresco to cover large areas.
* **Unlimited Length:** The veranda can be manufactured to any length to meet the needs of your customers.
* **Simple Fixing System with Minimal Parts:** The Whole Simplicity Alfresco range has been designed with ease of installation in mind, making it easier for your installation teams to fit saving time and money.
* **Integral Aluminium Guttering with Easy-Fix Profiles:** The integrated guttering creates a sleek, modern appearance which is stronger than external guttering systems and also means all cabling from extras such as lighting is hidden from view.
* **Available in any RAL or BS Colour:** The frame can be supplied in Anthracite Grey Textured (RAL 7016) as standard.
* **Optional Extras:** The Contemporary Alfresco veranda is available with many upgrades including integrated lighting, heaters, roof blinds (screener veranda) and glass doors, please see below for more information.

### Available Upgrades:

* **Infrared Heaters:** Wall Mounted Heaters and the option to have freestanding, can be added to create a gentle, ambient glow of heat underneath the veranda.
* With a modern look and a choice of 3 popular colours; black, silver and rose gold, to suit the heating and appearance requirements of the end user.
* **Integrated Lighting:** Integrated lighting can be added to the underside of the main bars and is hidden within the frame for a seamless appearance.
* The lighting features LED technology, making them economical to run, durable and not too bright or obtrusive.
* **Glass Room:** The Contemporary Alfresco is available with glass doors and fixed frames to create a fully enclosed Glass Room Upgrade.
* This upgrade features clear glass walls and sliding glass doors which are lockable.

### Alfresco Contemporary Standard Textured Colours:

* RAL 7016 Anthracite Grey Textured

| System Specs: |  |
| --- | --- |
| Max Projection | 6.0m |
| Max Span Between Posts | 6.0m |
| Minimum Pitch | 5 degrees |
| Maximum Pitch | 45 degrees |
| Roof Panel Type | 8mm glass |
| Max Gap between Roof Bars | 800mm  |
| Lighting Option | LED Strip Lighting |
| Upgrades Available | Glass Room, Glass Doors, Lighting, Heaters |
| Colour | RAL 7016 Anthracite Grey Textured |
| Drainage | Internal, within post |