The Simplicity 6 System

**A REVOLUTIONARY AND ELEGANT SYSTEM THAT’S QUICK AND EASY TO INSTALL**

*Ideal for Garden Verandas and Garden Canopies.*

The Simplicity 6 is a stylish veranda, canopy, carport and glass room system that is glazed with 6mm toughened glass.

With elegant posts and optional glass roofing, this product offers you a deluxe canopy or veranda at an affordable price.

By featuring the option of glass roofing, the Simplicity 6 offers improved acoustic properties – reducing the noise of raindrops during a downpour; these glass panels also provide a sparkling finish which is easy to maintain, particularly if you choose the self-cleaning glass.

The Simplicity 6 is the perfect veranda solution for domestic gardens and provides an effective and stylish cover from the weather for alfresco dining and garden parties.

With a projection of up to 3.5m from its supporting wall and an unlimited length, you will have a solution that can be adapted to suit your exact needs.

The Simplicity 6 comes with a full 10-year guarantee and a 60-year life expectancy, making this a real investment that you will be able to enjoy for many years to come.

* 3.5m Maximum Projection
* 4m Max Span Between Posts
* 800mm Max Between Bars
* 60 Years Life expectancy
* 10 Years Guarantee
* 3 Standard Colours
* 750mm Overhang to the Gutter & Wall Plate
* 22.5 Degrees Max Pitch
* 2.5 Degrees Mix Pitch

## 

## Why Sell The Simplicity 6 System To Your Customers?

**Full 10-Year Guarantee:** The Simplicity 6 is supplied with a full 10-year guarantee and a 60-year life expectancy for the canopy frame

**Glass:** The Simplicity 6 is covered with 6mm toughened glass or 6mm toughened, self-cleaning glass

**UV-Activated Self-Cleaning Glass:** The 6mm self-cleaning toughened glass has a UV-activated special coating that is applied during manufacture that breaks down organic dirt which is then washed away by the rain. Only a small amount of UV is needed to activate the special coating so that your canopy remains clean even on a cloudy day

**Toughened Glass:** Both glass options are toughened during manufacturing and achieve Class 1 BS EN 12600 for impact performance

**Glass:** 6mm toughened glass roof

**High Light Transmittance:** All roof options offer a high light transmittance

**Available Projections:** Up to 3.5 metres

**Low Maintenance:** All roof options are low maintenance, particularly the self-cleaning glass, which means less cleaning is required, saving you time and money

**Simple Fixing System with Minimal Parts:** For a simple and speedy installation

**Low Profile:** The Simplicity 6 can be fitted in height-restricted areas

**Integral Aluminium Guttering:** Creates a sleek, modern design which is stronger than external guttering systems and saves time on installation

**The Glass Room Upgrade:** The Simplicity 6 can be supplied with the glass room upgrade to offer your customers a completely enclosed garden room that can be used all year round

**Victorian Upgrade:** Available with the Victorian Upgrade

**Infrared Heaters:** Add Wall Mounted Infrared Heaters to your veranda to create a warm and cosy atmosphere

**Lighting:** Add stylish, efficient lighting for the complete finish, maximising the use of your canopy or veranda

## Available Upgrades:

**Infrared Heaters:** Wall Mounted Heaters and the option to have freestanding, can be added to create a gentle, ambient glow of heat underneath the veranda.

With a modern look and a choice of 3 popular colours; black, silver and rose gold, to suit the heating and appearance requirements of the end user.

**Integrated Lighting:** Integrated lighting can be added to the underside of the main bars and is hidden within the frame for a seamless appearance.

The lighting features LED technology, making them economical to run, durable and not too bright or obtrusive.

**Glass Room:** All Milwood Products can be used with glass doors and fixed frames to create a fully enclosed Glass Room Upgrade.

This upgrade features clear glass walls and sliding glass doors which are lockable.

**Victorian Upgrades:** The Victorian Upgrades can be added to create that traditional effect to keep in touch with the character of traditional buildings.

Decorative, Victorian-style upgrades can be used on the Simplicity 6, Simplicity 16, Simplicity 35 and Simplicity Xtra by using the 75 x 70 standard posts, which include base castings and gallows brackets.

**Simplicity 6 standard texture colours:**

* RAL 7016 Anthracite Grey Textured
* RAL 9005 Jet Black Textured

**Simplicity 6 Standard Semi-Gloss Colours:**

* RAL 9016 Traffic White Semi-Gloss

| **System Specs** |  |
| --- | --- |
| Max Projection | 3.5m |
| Mac Span Between Posts | 4.0 |
| Minimum Pitch | 2.5 degrees |
| Maximum Pitch | 22.5 degrees |
| Roof Panel Type | 6mm Glass |
| Max Gap Between Roof Bars | 800mm. Glass width is a maximum of 800mm up to 2m projection, over 2m – 700mm max up to 3m over 3m – 650mm |
| Lighting Option | LED Strip Lighting – AVAILABLE IN THE MAIN BARS AND GUTTER ONLY |
| Upgrades Available | Glass Room, Glass Doors, Lighting, Heaters, Victorian Upgrade |
| Colour | RAL 7016 Anthracite Grey Textured, RAL 9005 Jet Black Textured, RAL 9016 Traffic White Semi-Gloss |
| Drainage | Internal, External or Spigot Only |